{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":365,"n_cols":6,"rows_kept":365,"flags":["formulas_cached_only"]}
["辅助电源（D7 D8 ~220V）送电"]
["SSD590检测显示版本："]
["SSD590DRIVE"]
["ISSUE:X.XX"]
[null,"（按E键显示）"]
["DIGITAL DC DRIVE （数字直流系统）"]
["MENU LEVEL（菜单级）"]
[null,"（按M键显示主菜单）"]
["MENU LEVEL（菜单级）"]
[1,"DIAGNOSTICS（诊断）"]
[2,"SETUP PARAMETERS（参数设定）"]
[3,"PASSWORD（口令）"]
[4,"ALARM STAYUS（报警状态）"]
[5,"MENUS（菜单）"]
[6,"SETUP PARAMETERS(参数存放)"]
[7,"SERIAL LINKS（串行线路）"]
[8,"SYSTEM（系统）"]
["（按上升/下降键显示上/下一条指令，为循环指令。 按E键返回主菜单）"]
[]
["一：","MENU LEVEL（菜单级）"]
[null,"DIAGNOSTICS（诊断）"]
[null,null,"（按M键显示分菜单）"]
["DIAGNOSTICS（诊断）"]
["（按上升/下降键显示上/下一条指令，为循环指令。 按M键进入监测值， 按E键返回分菜单）"]
["序号","说明",null,"TAG  N","范围","监测值"]
[1,"SPEED DEMAND（速度要求）",null,89,"±105%",{"v":0,"d":"0.00%"}]
[2,"SPEED FEEDBACK（速度反馈）",null,207,"±150%",{"v":0,"d":"0.00%"}]
[3,"SPEED ERROR（速度误差）",null,297,"±150%",{"v":0,"d":"0.00%"}]
[4,"CURRENT DEMAND（电流要求）",null,299,"±200%",{"v":0,"d":"0.00%"}]
[5,"CURRENT FEEDBACK（电流反馈）",null,298,"±300%",{"v":0,"d":"0.00%"}]
[6,"POS. I CLAMP（正电流箱位）",null,87,"±200%",{"v":0,"d":"0.00%"}]
[7,"NEG. I CLAMP（负电流箱位）",null,88,"±200%",{"v":0,"d":"0.00%"}]
[8,"ACTUAL POS I LIM（总的正电流极限值）",null,67,"±200%",{"v":0,"d":"0.00%"}]
[9,"ACTUAL NEG I LIM（总的负电流极限值）",null,61,"±200%",{"v":0,"d":"0.00%"}]
[10,"INVERSE TIME O/P（及时限箱位输出电平）",null,203,"±0~200.00%",{"v":2,"d":"200.00%"}]
[11,"AT CURRENT LIMIT（处于电流极限）",null,42,"TRUE/FALSE",false]
[12,"AT ZERO SPEED（处于零速反馈）",null,77,"TRUE/FALSE",true]
[13,"AT ZERO SETPOINT（处于零速要求）",null,78,"TRUE/FALSE",true]
[14,"AT STANDSTILL（处于静止状态）",null,79,"TRUE/FALSE",true]
[15,"STALL TRIP（堵转跳闸）",null,112,"OK/INHIBITED","OK"]
[16,"RAMPING（斜坡）",null,113,"TRUE/FALSE",false]
[17,"PROGRAM STOP（程序停机）",null,80,"TRUE/FALSE",true]
[18,"DRIVE START（传动启动）",null,82,"ON/OFF","OFF"]
[19,"DRIVE ENABLE（传动允许）",null,84,"ENABLED/DISABLED","DISABLED"]
[20,"OPERATING MODE（运转方式）",null,212,"ON/STOP","STOP"]
[21,"FIELD ENABLE（励磁启动）",null,169,"ENABLED/DISABLED","DISABLED"]
[22,"FIELD DEMAND（励磁要求）",null,183,"0~+100%",{"v":0,"d":"0.00%"}]
[23,"FIELD I FBK（励磁电流反馈）.",null,300,"±125%",{"v":0,"d":"0.00%"}]
[24,"FLD.FIRING ANGLE（励磁触发角）",null,184,"5~155","0 DEG"]
[25,"ANIN 1(A2)（速度设定值1）",null,50,"±10V","0.00 VOLTS"]
[26,"ANIN 2(A3)（速度设定值2/电流要求）",null,51,"±10V","0.00 VOLTS"]
[27,"ANIN 3(A4)（速度设定值39斜坡）",null,52,"±10V","0.00 VOLTS"]
[28,"ANIN 4(A5)（负电流箱位）",null,53,"±10V","0.00 VOLTS"]
[29,"ANIN 5(A6)（正电流箱位或主电流极限）",null,54,"±10V","0.00 VOLTS"]
[30,"ANOUT 1(A7)（速度反馈输出）",null,55,"±10V","0.00 VOLTS"]
[31,"ANOUT 2(A8)（总速度设定值）",null,56,"±10V","0.00 VOLTS"]
[32,"START (C3)（起动运行）",null,68,"ON/OFF","OFF"]
[33,"JOG INPUT (C4)（总动输入）",null,69,"ON/OFF","OFF"]
[34,"ENABLE (C5)（允许工作）",null,70,"ON/OFF","OFF"]
[35,"DIGIN 1(C6)（对称电流箱位/不对称（ON=双极）",null,71,"ON/OFF","OFF"]
[36,"DIGIN 2(C7)（斜坡保持输入）",null,72,"ON/OFF","OFF"]
[37,"DIGIN 3(C8)（指示运转的速度或电流方式）",null,73,"ON/OFF","OFF"]
[38,"DIGOUT 1(B5)（处于零速）",null,74,"ON/OFF","ON"]
[39,"DIGOUT 2(B6)（传动装置正常）",null,75,"ON/OFF","ON"]
[40,"DIGOUT 3(B7)（传动装置准备好运行）",null,76,"ON/OFF","OFF"]
[41,"RAISE/LOWER O/P（上升/下降输出）",null,264,"±300%",{"v":0,"d":"0.00%"}]
[42,"PID OUTPUT（PID  输出）",null,417,"±315%",{"v":0,"d":"0.00%"}]
[43,"PID CLAMPED（PID  限幅）",null,416,"TRUE/FALSE",false]
[44,"PID ERROR（PID 误差）",null,415,"±105%",{"v":0,"d":"0.00%"}]
[45,"SPT SUM I OUTPUT（设定值加法器输出）",null,86,"±200%",{"v":0,"d":"0.00%"}]
[46,"RAMP OUTPUT（斜坡输出）",null,85,"±100%",{"v":0,"d":"0.00%"}]
[47,"SPEED SETPOINT（速度环总设定值）",null,63,"±150%",{"v":0,"d":"0.00%"}]
[48,"TERMINAL VOLTS（端电压）",null,57,"±125%",{"v":0,"d":"0.00%"}]
[49,"BACK EMF（电动机反电动势 IR补偿）",null,60,"±150%",{"v":0,"d":"0.00%"}]
[50,"TACH INPUT (B2)（测速发电机反馈）",null,308,"±110%",{"v":0,"d":"0.00%"}]
[51,"ENCODER（编码器反馈）",null,206,"±6000 RPM","0 RPM"]
[]
["二：","MENU LEVEL（菜单级）"]
[null,"SETUP PARAMETERS（参数设定）"]
[null,null,"（按M键显示分菜单）"]
["SETUP PARAMETERS（参数设定）"]
["（按上升/下降键显示上/下一条指令，为循环指令。按M键进入子菜单,按M键进入设定值,按E键返回上一级菜单）"]
[1," RAMP （斜坡）"]
[null,"序号","说明","TAG  N","范围","设定值"]
[null,"A","RAMP ACCEL TIME（斜坡加速时间）",2,"0.1~600.0S","10.0S"]
["（由零速到最高速的时间,A4输入）"]
[null,"B","RAMP DECEL TIME（斜坡减速时间）",3,"0.1~600.0S","10.0S"]
["（由最高速到零速的时间, A4输入）"]
[null,"C","CONSTANT ACCEL（恒加速）",4,"ENABLED/DISABLED","ENABLED"]
["（此条为欧陆口令文件  无）",{"$nulls":3},"(启动/禁止)"]
[null,"D","RAMP HOLD（斜坡保持）",118,"ON/OFF","ON"]
["（为真时斜坡输出保持在它的最后值，用RAMP RESET复位）",{"$nulls":3},"(开/关)"]
[null,"E","RAMP INPUT（斜坡输入）",5,"±100.00%",{"v":0,"d":"0.00%"}]
["（由A4端子作系统给定输入）"]
[]
[null,"F","%S—RAMP（%S-斜坡）",266,"0.1~100.0S",{"v":0.025,"d":"2.50%"}]
["（S形变化率的斜坡百分数，改变百分数影响斜坡时间及曲线）"]
[null,"G","RAMPING THRESH（斜坡阀值）",286,"0.1~100.0S",{"v":0.005,"d":"0.50%"}]
["（斜坡标志阀值电平，阀值用以检测斜坡是否有效）"]
[null,"H","AUTO RESET（自动复位）",287,"ENABLED/DISABLED","ENABLED"]
["（如自动复位启动，只要系统复位为真，斜坡便复位）",{"$nulls":3},"(启动/禁止)"]
[null,"I","EXTERNAL RESET（外部复位）",288,"ENABLED/DISABLED","DISABLED"]
["（如外部复位启动，斜坡便保持为复位状态。外部复位与自动复位无关）",{"$nulls":3},"(启动/禁止)"]
[null,"J","RESET VALUE（复位值）   ",422,"±300.00%",{"v":0,"d":"0.00%"}]
["（在斜坡复位为真或通电时，预先装入输出端，为使速度平滑过度既无冲击，与速度反馈 62 连接）"]
[null,"K","MIN SPEED（最小速度）",126,"0.1~100.0S",{"v":0,"d":"0.00%"}]
["（最小速度是双向的，工作时有0.5%的滞后，用以斜坡输入）"]
[]
[2,"AUX I/O（辅助输入/输出）"]
[null,"A","AUX START（辅助起动）",161,"ON/OFF","ON"]
["（由C3加+24V，控制软件起动/运行指令）"]
[null,"B","AUX JOG（辅助点动）",227,"ON/OFF","ON"]
["（由C4加+24V，控制软件点动指令）"]
[null,"C","AUX ENABLE（辅助允许）",168,"ON/OFF","ON"]
["（由C5加+24V，控制软件允许指令）"]
[null,"D","AUX DIGOUT1（辅助数字输出1）",94,"ON/OFF","OFF"]
[null,"E","AUX DIGOUT2（辅助数字输出2）",95,"ON/OFF","OFF"]
[null,"F","AUX DIGOUT3（辅助数字输出3）",96,"ON/OFF","OFF"]
[null,"G","ANOUT1（模拟输入1）",128,"±100.00%",{"v":0,"d":"0.00%"}]
[null,"H","ANOUT2（模拟输入2）",129,"±100.00%",{"v":0,"d":"0.00%"}]
[]
[3,"JOG/SLACK（点动/放松）"]
[null,"A","JOG SPEED1（点动速度 1）",218,"±100.00%",{"v":0.05,"d":"5.00%"}]
["（用以设定系统正向点车速度）"]
[null,"B","JOG SPEED2（点动速度 2）",219,"±100.00%",{"v":-0.05,"d":"-5.00%"}]
["（用以设定系统反向点车速度）"]
[null,"C","TAKE UP1（启动 1）",253,"±100.00%",{"v":0.05,"d":"5.00%"}]
["(启动速度设定值1)"]
[null,"D","TAKE UP2（启动 2）",254,"±100.00%",{"v":-0.05,"d":"-5.00%"}]
["(启动速度设定值2)"]
[null,"E","CRAWL SPEED（爬行速度）",225,"±100.00%",{"v":0.1,"d":"10.00%"}]
["（爬行速度设定值）"]
[null,"F","MODE（方式）",228,"TRUE/FALSE",false]
["（用以设定点动/启动工作方式）",{"$nulls":3},"(真/虚)"]
[null,"G","RAMP RATE（斜坡速率）",355,"0.1~600.00S","1.0S"]
["（点动与主斜坡速率无关，用以设定点动斜坡速率）"]
[]
[4,"RASET/LOWER（上升/下降）"]
[null,"A","RESET VALUE（复位值）",255,"±300%",{"v":0,"d":"0.00%"}]
["（此值在外部复位为真或通电时预先装入输出端，由最大和最小值箝位）"]
[null,"B","INCREASE RATE（增加速率）",256,"0.1~600.00S","10.0S"]
["（由零速到最高速的变化速率既时间）"]
[null,"C","DECREASE RATE（减少速率）",257,"0.1~600.00S","10.0S"]
["（由最高速到零速的变化速率既时间）"]
[null,"D","RAISE INPUT（上升输入）",261,"TRUE/FALSE",false]
["（提高输出的指令）",{"$nulls":3},"(真/虚)"]
[null,"E","LOWER INPUT（下降输入）",262,"TRUE/FALSE",false]
["（降低输出的指令）",{"$nulls":3},"(真/虚)"]
[null,"F","MIN VALUE（最小值）",258,"±100.00%",{"v":-1,"d":"-100.00%"}]
["（最小斜坡输出箝位值，是平坦箝位，不是成斜坡的最小速度设定值）"]
[null,"G","MAX VALVE（最大值）",259,"±100.00%",{"v":1,"d":"100.00%"}]
["（最大斜坡输出箝位值）"]
[null,"H","EXTERNAL RESET（外部复位）",307,"TRUE/FALSE",false]
["（如外部复位为真，上升/下降组件的输出便设定为复位值）",{"$nulls":3},"(真/虚)"]
[]
[5,"SPECLAL BLOCKS（专用模快）"]
["（用以具有线性控制要求的场合，如冶金，纺织，造纸，印刷等行业）"]
[]
[6,"FIELD CONTROL（励磁控制）"]
[null,"A","FIELD ENABLE（励磁启动）",170,"ENABLED/DISABLED","ENABLED"]
["（如使用590内部励磁设置启动，如外加励磁或为永磁电机设置禁止）",{"$nulls":3},"(启动/禁止)"]
[null,"B","FLD CTRL MODE IS（励磁控制方式）",209,"VOLTAGE/CURRENT","VOLTAGE"]
["（用以选择电压VOLTAGE/电流CURRENT控制方式，建议选用电流方式）",{"$nulls":3},"(电压/电流)"]
[null,"C","FLD VOLTAGE VARS（励磁电压变量）"]
[null,null,"1.RATIO OUT/IN（输入/输出比率）",210,"0.00~100.00%",{"v":0.9,"d":"90.00%"}]
["（电压控制既开环控制励磁的输出电压，为系统设定比率）"]
[null,"D","FLD CURRENT VARS（励磁电流变量）"]
[null,null,"1.SETPOINT（励磁电流设定量）",171,"0.00~100.00%",{"v":1,"d":"100.00%"}]
["（根据励磁电流设定，设定励磁电流值）"]
[null,null,"2.PROP.GAIN（比例增益）",173,"0.00~100.00%",0.1]
["（励磁电流回路PI的比例增益，比例大反应快，易振荡，过冲）"]
[null,null,"3.INT.GAIN（积分增益）",172,"0.00~100.00%",1.28]
["（励磁电流回路PI的积分增益，积分大反应慢，周期长）"]
[null,null,"4.FLD WEAR VARS（励磁弱磁变量）"]
[null,null,"A.FLD WEAR ENABLE(励磁弱磁启动）",174,"ENABLED/DISABLED","DISABLED"]
["（弱磁启动为弱磁升速而设定，弱磁不启动励磁弱磁不工作）",{"$nulls":3},"(启动/禁止)"]
[null,null,"B.EMF LEAD（电动势超前项 T1）",175,"0.00~100.00%",2]
[null,null,"C.EMF LAG（电动势滞后项 T2）",176,"0.00~100.00%",40]
[null,null,"D.EMF GAIN（电动势增益 KP）",177,"0.00~100.00%",0.3]
[null,null,"E.MIN FLD CURRENT（最小励磁电流）",179,"0.00~100.00%",{"v":0.1,"d":"10.00%"}]
["（设定弱磁后最小励磁电流）"]
[null,null,"F.MAX VOLTS（最大电压）",178,"0.00~100.00%",{"v":1,"d":"100.00%"}]
["（设定弱磁转换点电压）"]
[null,null,"G.BEMF FBK LEAD（反电动势反馈超前）",191,"10-5000ms","100ms"]
["（反电动势反馈滤波器的超前时间常数）"]
[null,null,"H.BEMF FBK LAG（反电动势反馈滞后）",192,"10-5000ms","100ms"]
["（反电动势反馈滤波器的滞后时间常数）"]
[null,"E","FLD QUENCH DELAY（励磁中止延时）",185,"0.0~600.0S","0.0S"]
["（在传动系统C3断电后，励磁维持时间）"]
[null,"F","FLD QUENCH MODE（励磁中止方式）",186,"QUENCH/STANDBY","QUENCH"]
["（在传动系统C3断电后，励磁中止控制方式，中止=0，备用=50%）",{"$nulls":3},"(中止/备用)"]
[7,"CURRENT PROFILE（电流曲线）"]
[null,"A","SPD BRK1 (LOW)（速度中断点1）",32,"0.00~100.00%",{"v":1,"d":"100.00%"}]
["（速度中断点1是电流极限曲线开始处的电动机速度）"]
[null,"B","SPD BRK2 (HIGH)（速度中断点2）",31,"0.00~100.00%",{"v":1,"d":"100.00%"}]
["（速度中断点2是电流极限曲线结束处的速度上限）"]
[null,"C","IMAX BRK1 (SPD1)（最大电流断续点1）",93,"0.00~100.00%",{"v":2,"d":"200.00%"}]
["（最大电流断续点1对应速度中断点1）"]
[null,"D","IMAX BRK2 (SPD2)（最大电流断续点2）",33,"0.00~100.00%",{"v":2,"d":"200.00%"}]
["（最大电流断续点2对应速度中断点2）"]
[]
[8,"STOP RATES（停机速率）"]
[null,"A","STOP TIME（停机时间）",27,"0.1~600.0S","10.0S"]
["（C3断电从100%设定速度到零速的时间）"]
[null,"B","STOP LIMIT（停机极限）",217,"0.0~600.0S","60.0S"]
[null,"C","CONTACTOR DELAY（接触器延时）",302,"0.1~600.0S","1.0S"]
["（控制D7，D8输出电压的延时时间）"]
[null,"D","PROG STOP TIME（程序停机时间）",26,"0.1~600.0S","0.1S"]
[null,"E","PROG STOP LIMIT（程序停机极限）",216,"0.0~600.0S","60.0S"]
[null,"F","PROG STOP ILIM（程序停机电流极限）",91,"0.00~200.00%",{"v":1,"d":"100.00%"}]
[null,"G","STOP ZERO SPEED（停机零速）",29,"0.0~100.00%",{"v":0.02,"d":"2.00%"}]
["（程序停机和一般停机方式下零速电平，控制接触器延时C）"]
[]
[9,"CALIBRATION（校准）"]
[null,"A","ARMATURE V CAL（电枢电压校准）",20,"0.9800~1.1000",1]
["(所需有效电压值处精确显示100%的电动机电枢电压的修整调节)"]
[null,"B","IR COMPENSATION（IR 补偿）",21,"0.00~100.00%",{"v":0,"d":"0.00%"}]
["（电枢电压反馈作速度反馈时，补偿电动机IR压降，改进调节防止电枢电压）"]
[null,"C","ENCODER RPM（编码器 转/分）",22,"0~6000 RPM","1000RPM"]
["(使用编码器反馈时电动机最高速度设定值)"]
[null,"D","ENCODER LINES（编码器 线）",24,"10~5000",1000]
["(标准的5701微测速机,每转有1000条线)"]
[null,"E","ANALOG TACH CAL（模拟测速机校准）",23,"0.9800~1.100",1]
["(在所需实际速度值处修整调节电动机速度使之精确显示100%,1500转/分为例)"]
[null,"F","ZERO SPD.OFFSET（零速偏置）",10,"±5.00%",{"v":0,"d":"0.00%"}]
["(如在传动稳定时速度反馈不为0,设定这一参数使速度反馈读数为零)"]
[null,"G","ARMATURE I (A9)（电枢电流 A9）",25,null,"BIPOLAR"]
["(用以选择电流表输出,双极或单极)"]
[null,"H","SPDFBK ALM LEVEL（速度反馈报警电平）",180,"0.0~100.0%",{"v":0.5,"d":"50.00%"}]
["(速度反馈报警比较速度反馈与电枢电压,报警电平是为了驱动报警,这二个信号之差应超过设定值)"]
[null,"I","STALL THRESHOLD（堵转阀值）",263,"0.00~200.00%",{"v":0.95,"d":"95.00%"}]
["(堵转比较电流反馈的阀值电平)"]
[null,"J","STALL TRIP DELAY(堵转跳闸延时）",224,"0.1~600.0S","10.0S"]
["(堵转输出成为真之前,堵转比较器的超时延时)"]
[null,"K","OVER SPEED LEVEL（超速报警）",188,"0.00~200.00%",{"v":1.25,"d":"125.00%"}]
["(超速报警的速度反馈电平)"]
[null,"L","FIELD I CAL（励磁电流校准）",182,"0.9800~1.1000",1]
["(在所需的有效电流值处用以修整调节电动机励磁电流,以精确显示100%)"]
[10,"INHIBIT ALARMS（禁止报警）"]
[null,"A","FIELD FAIL（励磁故障）",19,"ENABLED/INHIBITED","ENABLED"]
[{"$nulls":4},"(启动/禁止)"]
[null,"B","5703 RCV ERROR（5703接收误差）",111,"ENABLED/INHIBITED","ENABLED"]
[{"$nulls":4},"(启动/禁止)"]
[]
[null,"C","STALL TRIP（堵转跳闸）",28,"ENABLED/INHIBITED","INHIBITED"]
[{"$nulls":4},"(启动/禁止)"]
[null,"D","TRIP RESET（跳闸复位）",305,"TRUE/FALSE",true]
[{"$nulls":4},"(真/虚)"]
[null,"E","SPEED FBK ALARM（速度反馈报警）",81,"ENABLED/DISABLED","ENABLED"]
[{"$nulls":4},"(启动/禁止)"]
[null,"F","ENCODER ALARM（编码器报警） ",92,"ENABLED/DISABLED","ENABLED"]
[{"$nulls":4},"(启动/禁止)"]
[11,"CURRENT LOOP（电流环）"]
[null,"A","CUR  LEMIT/SCALER（电流限幅定标）",15,"0.00~200.00%",{"v":1,"d":"100.00%"}]
["（电流极限定标器定标双极/单极的箝位值）"]
[null,"B","MAIN CURR .LIMIT（主电流极限）",421,"0.00~200.00%",{"v":2,"d":"200.00%"}]
["（主电流极限参数与电流极限定标器无关，与另外3个电流极限模块串联）"]
[null,"C","PROP.GAIN（比例增益）",16,"0.00~200.00%",{"v":0.45,"d":"45.00%"}]
["(电枢电流PI回路的比例增益控制参数,大反应快,振荡.在自动调谐中设定)"]
[null,"D","INT.GAIN（积分增益）",17,"0.00~200.00%",{"v":0.035,"d":"3.50%"}]
["(电枢电流PI回路的积分增益控制参数,大反应快,振荡.在自动调谐中设定)"]
[null,"E","AUTO TUNE（自动调谐）",18,"ON/OFF","OFF"]
["(自动调谐功能的触发器输入)"]
[null,"F","DISCONTINUOUS（断续点）",137,"0.00~200.00%",{"v":0.12,"d":"12.00%"}]
["(电枢电流断续到连续的分界点,在自动调谐中设定,影响自适应算法的性能)"]
[null,"G","ADDITIONAL DEM（附加给定）",30,"±200.00%",{"v":0,"d":"0.00%"}]
["(附加电流给定输入)"]
[null,"H","BIPOLAR CLAMPS（双极箝位）",90,"ENABLED/DISABLED","DISABLED"]
["(为4象限运转选择双极不对称或单极对称电流箝位的输入)",{"$nulls":3},"(启动/禁止)"]
[null,"I","REGEN MODE（再生方式）",201,"ENABLED/DISABLED","ENABLED"]
["(再生4象限或非再生2象限运转方式的选择输入端)",{"$nulls":3},"(启动/禁止)"]
[null,"J","POS.I CLAMP（正电流箝位）",301,"±200%",{"v":1,"d":"100.00%"}]
["(双极箝位方式中的正电流箝位)"]
[null,"K","NEG.I CLAMP（负电流箝位）",48,"±200.00%",{"v":-1,"d":"-100.00%"}]
["(双极箝位方式中的负电流箝位)"]
[null,"L","I DMD .ISOLATE（电流给定隔离）",119,"ENABLED/DISABLED","DISABLED"]
["(速度环旁路,该电流给定取自模拟输入端2-A3)",{"$nulls":3},"(启动/禁止)"]
[12,"SPEED LOOP（速度环）"]
[null,"A","PROP.GAIN（比例增益）",14,"0.00~200.00%",10]
["(速度环PI回路的比例增益调节参数,大反应快,振荡)"]
[null,"B","INT.TIME CONST（积分时间常数）",13,"0.00~200.00%","0.500S"]
["(速度环PI回路的积分增益调节参数,大反应快,振荡)"]
[null,"C","INT.DEFEAT（积分失效）",202,"ON/OFF","OFF"]
["(禁止速度环PI控制的积分部份,仅用比例控制)"]
[null,"D","ENCODER SIGN（编码器符号）",49,"POSITIVE/NEGATIVE","POSITIVE"]
["(编码器反馈不能电气反向,仅用控制软件使信号极性反向)",{"$nulls":3},"(正/负)"]
[null,"E","SPEED FBK SELECT（速度反馈选择）",47,null,"ARM VOLTS FBK"]
[null,null,"1.ARM VOLTS FBK（电枢电压反馈）"]
[null,null,"2.ANALOG TACH（模拟测速机反馈）"]
[null,null,"3.ENCODER（编码器反馈）"]
[null,null,"4.ENCODER/ANALOG（编码器/模拟测速机反馈组合）"]
[]
[null,"F","ADVANCED（先进的）"]
[null,null,"1.ADAPTION（先进的自适应功能）"]
[null,null,"A.MODE（方式）",268,"0~3",0]
[null,null,"    0-禁止"]
[null,null,"    1-与速度反馈有关"]
[null,null,"    2-与速度误差有关"]
[null,null,"    3-与电流要求有关"]
[null,null,"B.SPD BRK1 (LOW)（速度中断点1 低）",269,"0.00~200.00%",{"v":0.01,"d":"1.00%"}]
[null,null,"（如方式=1 中断点与速度反馈对应）"]
[null,null,"（如方式=2 中断点与速度误差对应）"]
[null,null,"（如方式=3 中断点与电流要求对应）"]
[null,null,"C.SPD BRK2 (HIGH)（速度中断点2 高）",270,"0.00~200.00%",{"v":0.05,"d":"5.00%"}]
[]
[null,null,"D.PROP.GAIN（比例增益）",271,"0.00~200.00%",{"v":0.05,"d":"5.00%"}]
[null,null,"(比例增益用于速度中断点1以下)"]
[null,null,"E.INT.TIME CONST（积分时间常数）",272,"0.00~200.00%",{"v":0.005,"d":"0.50%"}]
[null,null,"(积分时间常数用于速度中断1之下)"]
[null,null,"2.I GAIN IN RAMP（斜坡电流增益）",274,"0.00~200.00%",1]
["(在斜坡标记号113为真时,积分增益由斜坡电流增益换算,用以防止装置处于斜时积分结束)"]
[null,null,"3.POS.LOOP P GAIN（位置环比例增益）",273,"0.00~200.00%",{"v":0,"d":"0.00%"}]
[]
[null,null,"4.I COMP（电流补偿）",275,"0.00~200.00%",{"v":0,"d":"0.00%"}]
[]
[null,null,"5.ZERO SPD.QUENCH（零速断开）"]
[null,null,"A.ZERO SPD LEVEL（零速电平）",284,"0.00~200.00%",{"v":0.005,"d":"0.50%"}]
["(速度要求和速度反馈的阀值)"]
[null,null,"B.ZERO LAD LEVEL（零电流电平）",285,"0.00~200.00%",{"v":0.015,"d":"1.50%"}]
["(电流要求阀值)"]
[null,"G","SETPOINTS（设定值）"]
[null,null,"A.SETPONT 1（设定点 1）",289,"±100%",{"v":0,"d":"0.00%"}]
["（速度设定点 1）"]
[null,null,"B.SIGN 2 (A3)（符号 2）",9,"POSITIVE/NEGATIVE","POSITIVE"]
["（速度设定点2的符号）",{"$nulls":3},"(正/负)"]
[null,null,"C.RATIO 2 (A3)（比率 2）",7,"±3.0000",1]
["（速度设定点2的比率）"]
[null,null,"D.SETPOINT 2 (A3)（设定点 2）",290,{"v":1,"d":"100%"},{"v":0,"d":"0.00%"}]
["（速度设定点2的固定设定点，不可组态，与电流环同步被扫描 ）"]
[null,null,"E.SETPOINT 3（设定点 3）",291,{"v":1,"d":"100%"},{"v":0,"d":"0.00%"}]
["（速度设定点 3，来自斜坡输出）"]
[null,null,"F.SETPONT 4（设定点 4）",41,{"v":1,"d":"100%"},{"v":0,"d":"0.00%"}]
["（速度设定点 4，来自5703输入）"]
[null,null,"G.MAX DEMAND（最大给定）",357,"0~105.00%",{"v":1.05,"d":"105.00%"}]
[null,null,"H.MIN DEMAND（最小给定）",358,"0~-105.00%",{"v":-1.05,"d":"-105.00%"}]
[]
[13,"STANDSTILL（静止）"]
[null,"A","STANDSTILL LOGIC（静止逻辑）",11,"ENABLED/DISABLED","DISABLED"]
["(在零设定值和零速禁止控制器就是处于静止状态,防止倒转)",{"$nulls":3},"(启动/禁止)"]
[null,"B","ZERO  THRESHOLD（零阀值）",12,"0.00~100.00%",{"v":0.02,"d":"2.00%"}]
["(零设定值和零速诊断输出的阀值电平控制零速继电器输出)"]
[null,"C","SONRCE TAG （源标记号  无）",306,"0~499",89]
[14,"SETPOINT SUM1(设定点合计1)"]
[null,"A","RATIO 1(比率1)",6,"±3.0000",1]
["(模似输入1的换算)"]
[null,"B","RATIO 0(比率0)",208,"±3.0000",1]
["(模似输入0的换算)"]
[null,"C","SIGN 1(符号1)",8,"POSITIVE/NEGATIVE","POSITIVE"]
["(模似输入1的极性)",{"$nulls":3},"(正/负)"]
[null,"D","SIGN 0(符号0)",292,"POSITIVE/NEGATIVE","POSITIVE"]
["(输入0的极性)",{"$nulls":3},"(正/负)"]
[null,"E","DIVIDER 1(除法1)",419,"±3.0000",1]
["(模似输入1的换算)"]
[null,"F","DIVIDER 0(除法0)",420,"±3.0000",1]
["(输入0的换算)"]
[null,"G","DEADBAND WIDTH(死区宽度-非灵敏区)",131,"0.0~100.00%",{"v":0,"d":"0.00%"}]
["(模似输入1的死区宽度)"]
[null,"H","LIMIT(极限)",375,"0~200.00%",{"v":1.05,"d":"105.00%"}]
["(设定点合计的可编程极限,是对称的,该极限适用于比率计算的中间结果和总输出)"]
[null,"I","INPUT 2(输入2)",423,"±200.00%",{"v":0,"d":"0.00%"}]
["(系统预设这一输入端不于任何模似输入连接)"]
[null,"J","INPUT 1(输入1)",100,{"v":2,"d":"200.00%"},{"v":0,"d":"0.00%"}]
["(系统预设这一输入端与模似输入1连接)"]
[null,"K","INPUT 0(输入0)",309,"±200.00%",{"v":0,"d":"0.00%"}]
["(系统预设这一输入端不于任何模似输入连接)"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}